# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of Catamaran, Powerboat with a trailer and Kayak trailer for the project BAJA- SOMBOR TOURISM4ALL p 1/3**

**Publication reference:** **HUSRB/1903/31/0075-5/catamaran, powerboat and trailer 6.1.2; 6.1.3 and 6.1.4**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

**Lot no. 1 - Catamaran**

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Catamaran** with next characteristics **– 1 pc:**  - Two hull vessel (catamaran)  - Efficient, speed min. 16 km/h with engines power up to 20 hp  - The purpose of the vessel is sports and recreation for the transport of up to 12 people, adapted and equipped for the transport of people with special needs and the disabled  - Hull material: fiberglass composite composed of aluminum pipes and aluminum substructure, with anti-slip floor and ramps for easy access to the vessel  - Overall dimensions: width 4.8-5.0 m; length 9.0-10.0 m (without motor)  - Catamaran with roof and railing, with two engines of at least 9.8 hp and a control console |  |  |  |
|  | Delivery place must be Trg cara Uroša no. 1, 25000 Sombor |  |  |  |
|  | Warranty period must be min. 2 (two) years from the date of provisional acceptance |  |  |  |

**Lot no. 2 – Powerboat with a trailer and Kayak trailer**

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Boat, outboard engine** **and motorboat trailer** with next characteristics – **1 set**:  A) Boat:  - Material: three-layer polietilen "schock-resistant"  - Number of persons: 5  - Length: 4.5 meters  - Width: 1.8 meters  - Steering wheel control  - Engine power: 20 to 40 hp  - Self-emptying boat trough  B) Outboard engine  - Four-stroke engine  - Power: 30 hp  - With electric injection and hydraulic trim  - Number of cylinders: 3  - Volume: from 500 cm3 to 530 cm3  - Weight: up to 75 kg  C) Motorboat trailer  - Load capacity: up to 750 kg  - Trailer must be galvanized with rollers and winch  - Trailer must have all the technical documentation for the registration as trailer adequate for public traffic |  |  |  |
| **2** | **Kayak trailer** with next characteristics – **1 pc**:  - Load capacity: up to 750 kg  - intended for the transport of 16 single-seater or two-seater kayaks  - Trailer must have all the technical documentation for the registration as trailer adequate for public traffic |  |  |  |
|  | Delivery place must be Trg cara Uroša no. 1, 25000 Sombor |  |  |  |
|  | Warranty period must be min. 2 (two) years from the date of provisional acceptance |  |  |  |